# Micro-Manager/μMANAGER/ImageJ

1. Please copy the corresponding dynamic library files (.dll, .dylib, or .so) to the installation directory of micro-manager according to the OS platform. For Windows and Linux platform, please copy library files in x86 folder for 32bit OS and copy library files in x64 foder for 64bit OS.

- Windows: copy mmgr_dal_MiiCam.dll and miicam.dll into the installation directory of micro-manger.
- MacOS: copy libmmgr_dal_MiiCam and libmiicam.dylib into the installation directory of micro-manager.
- Linux: copy libmmgr_dal_MiiCam.so.0 and libmiicam.so into the installation directory of micro-manager.

2. Please pay attention to the "Device API Version" of micro-manager, such as 68, 69, 70, 71, etc. You can find the "Device API Version" in the About box of micro-manager (See the image below). Then, select file in the matching sub-directory according to the "Device API Version" of micro-manager. Using mismatch version file cause the software to not work properly or even crash.

3. To use the camera, you can add the camera into the current configuration or create a new configuration. In the hardware configuration wizard, you can find the camera as MiiCam in the available device list. Add MiiCam in the device list and then you can use it in micro-manager.